|  |  |  |
| --- | --- | --- |
| 2 |  |  |
| 4 |  |  |
| 6 | Drive select 3 |  |
| 8 | Index |  |
| 10 | Drive select 0 |  |
| 12 | Drive select 1 |  |
| 14 | Drive select 2 |  |
| 16 | Motor on |  |
| 18 | Dierction |  |
| 20 | STEP |  |
| 22 | WRITE DATA |  |
| 24 | WRITE enable |  |
| 26 | Track 00 |  |
| 28 | Write protect |  |
| 30 | READ DATA |  |
| 32 | SIDE select |  |
| 34 |  |  |